Hyun-Woo Kim   Senior Electrical Engineer
Ann Arbor, MI  ·  hyunwoo.kim@gmail.com  ·  +1 734-555-0189  ·  linkedin.com/in/hyunwookim
PROFILE SUMMARY
· Senior Electrical Engineer with 7 years in EV power electronics, now designing onboard charger hardware at Rivian after almost 3 years on 48 V and 12 V power boards at General Motors.
· Designs in Altium Designer, models in Simulink, PLECS and LTspice, checks parasitics in Ansys Q3D, and automates bench and HIL tests in LabVIEW and Python.
· Strong in SiC power stages, totem-pole PFC, isolated gate drives and EMI filter design, with parts picked to AEC-Q100 and AEC-Q101 grades and a second source wherever one exists.
· Works with controls firmware, thermal and vehicle integration teams through B-sample and C-sample builds, and owns the charger’s interface spec with the battery team.
· Mentors 2 engineers on gate drive layout, co-leads the power electronics design review, and wrote the team’s SiC double-pulse test guide.
TECHNICAL SKILLS
Schematic & PCB Tools:	Altium Designer, Altium 365, Xpedition (GM programs)
Simulation & Analysis:	Simulink, PLECS, LTspice, Ansys Q3D, MATLAB
Power Conversion:	Totem-pole PFC, CLLC and LLC converters, SiC MOSFETs, isolated gate drivers, 48 V DC-DC, EMI filters
Analog & Signal Chain:	Shunt and Hall current sensing, isolated amplifiers, 16-bit ADCs, active filters
Interfaces & Microcontrollers:	CAN FD, SPI, TI C2000, Infineon AURIX (hardware side)
Lab & Test Equipment:	Yokogawa WT5000, double-pulse test rig, LabVIEW HIL benches, thermal chambers, Python
Compliance Standards:	CISPR 25, ISO 7637-2, ISO 16750, AEC-Q100, AEC-Q101, ISO 26262 hardware metrics
EDUCATION
University of Michigan   M.S. in Electrical and Computer Engineering	Ann Arbor, MI · Sep 2017 to May 2019
WORK EXPERIENCE
Rivian   Senior Electrical Engineer, Power Electronics	Plymouth, MI · Mar 2022 to Present
· Led the power stage design of the onboard charger’s totem-pole PFC and CLLC stages on SiC MOSFETs, raising peak efficiency from 94.8% to 96.6% at full load.
· Designed the gate driver and isolated sensing board in Altium Designer, choosing AEC-Q100 parts with a second source for every IC, which cut the board’s BOM cost by $6.80 a unit.
· Built Simulink and PLECS models of the PFC current loop and matched them to bench data within 3%, so controls could try loop changes in simulation before touching a board.
· Cut the charger’s conducted emissions with a two-stage EMI filter and a new common-mode choke, clearing CISPR 25 Class 5 limits with 6 dB of margin on the first chamber visit.
· Brought up B-sample chargers on a LabVIEW HIL bench with a Yokogawa WT5000, running thermal and line-sag profiles that found 9 faults before vehicle testing began.
General Motors   Electrical Engineer	Warren, MI · Jul 2019 to Feb 2022
· Reviewed the layout of a 48 V mild hybrid DC-DC board with the PCB team, moving the power loop onto inner layers and cutting switch-node overshoot from 22 V to 9 V.
· Designed current sensing for a 12 V battery monitor with a shunt and a 16-bit ADC, holding measurement error under 0.5% from -40°C to 105°C.
· Ran DFM reviews with the Tier 1 supplier on 2 vehicle programs and closed 31 ECOs, raising end-of-line test yield from 95.2% to 98.7%.
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